**Hygrostat HY 5 I**

Hygrostat for controlling fans depending on the relative air humidity.

With internal scale - therefore protected against accidental resetting.

Maximum current with inductive load: 5.0 A for dehumidifying, 2.2 A for humidifying.

Application areas: Laundries and other humid areas.

Continuous setting range: 20% to 80% relative humidity.

Switching hysteresis: Approx. 8 % relative humidity.

It is possible to operate the fan with increasing or decreasing humidity selected.

Technical data

|  |  |
| --- | --- |
| Article: | HY 5 I |
| Frequency: | 50 Hz/60 Hz |
| Colour: | Pure white, similar to RAL 9010 |
| Weight: | 0,1 kg |
| Weight including packaging: | 0,233 kg |
| Width: | 132 mm |
| Height: | 82 mm |
| Depth: | 40 mm |
| Width with packaging: | 137 mm |
| Height with packaging: | 55 mm |
| Depth with packaging: | 90 mm |
| Operating element: | Interior |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799571254 |
| Article number: | 0157.0125 |

Manufacturer: MAICO

HY 5 I Hygrostat