**Radio receiver XE 1**

Radio receiver for a wireless connection from the switch to the fan.

Installation in standard recessed-mounting box or distribution box.

Radio system consists of XS 1 radio switch and at least one XE 1 radio receiver.

An XS 1 can be assigned any number of XE 1.

Technical data

|  |  |
| --- | --- |
| Article: | XE 1 |
| Type of voltage: | Alternating current |
| Rated voltage: | 230 V |
| Maximum load (inductive load): | 2 A |
| Maximum load (ohmic load): | 4 A |
| Degree of protection: | IP 20 |
| Type of installation: | Recessed-mounted |
| Colour: | Blue |
| Weight: | 0,05 kg |
| Weight including packaging: | 0,08 kg |
| Width: | 52 mm |
| Height: | 52 mm |
| Depth: | 21 mm |
| Width with packaging: | 80 mm |
| Height with packaging: | 80 mm |
| Depth with packaging: | 45 mm |
| Ambient temperature: | 55 °C |
| Radio frequency: | 433 MHz |
| Number of radio channels: | 1 Channel |
| Programmable transmitter/switch: | 14 |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799573432 |
| Article number: | 0157.0343 |

Manufacturer: MAICO

XE 1 Radio receiver