**Step switch, reversing switch FS 6**

FS 6: 2-step reversing switch for ventilation and air extraction.

Technical data

|  |  |
| --- | --- |
| Article: | FS 6 |
| Air direction: | Ventilation / Air extraction |
| Type of voltage: | Alternating current |
| Rated voltage: | 230 V |
| Frequency: | 50 Hz |
| Maximum load (inductive load): | 0,35 A |
| Degree of protection: | IP 20 |
| Type of installation: | Surface-mounted |
| Colour: | Pearl white, similar to RAL 1013 |
| Weight: | 0,38 kg |
| Weight including packaging: | 0,4 kg |
| Width: | 128 mm |
| Height: | 74 mm |
| Depth: | 46 mm |
| Width with packaging: | 130 mm |
| Height with packaging: | 78 mm |
| Depth with packaging: | 52 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799161066 |
| Article number: | 0016.0106 |

Manufacturer: MAICO

FS 6 Step switch, reversing switch