**Reversing switch W 1**

Reversing switch for fan control.

For alternating air direction.

WU 1: With switch box for recessed mounting.

Technical data

|  |  |
| --- | --- |
| Article: | W 1 |
| Air direction: | Ventilation and air extraction |
| Type of voltage: | Alternating current / Three-phase AC |
| Rated voltage: | 230 V / 400 V |
| Frequency: | 50 Hz/60 Hz |
| Maximum load: | 16 A |
| Degree of protection: | IP 65 |
| Type of installation: | Surface-mounted |
| Colour: | Light grey |
| Weight: | 0,37 kg |
| Weight including packaging: | 0,4 kg |
| Width: | 82 mm |
| Height: | 82 mm |
| Depth: | 127 mm |
| Width with packaging: | 95 mm |
| Height with packaging: | 88 mm |
| Depth with packaging: | 133 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799571018 |
| Article number: | 0157.0101 |

Manufacturer: MAICO

W 1 Reversing switch