**Pole-changing switch P 1**

Pole-changing switch for controlling pole-changeable fans.

Step switch for 2 speeds.

Technical data

|  |  |
| --- | --- |
| Article: | P 1 |
| Type of voltage: | Three-phase AC |
| Rated voltage: | 500 V |
| Maximum load: | 16 A |
| Degree of protection: | IP 65 |
| Motor: | Dahlander circuit |
| Type of installation: | Surface-mounted |
| Weight: | 0,4 kg |
| Weight including packaging: | 0,43 kg |
| Width: | 82 mm |
| Height: | 82 mm |
| Depth: | 127 mm |
| Width with packaging: | 95 mm |
| Height with packaging: | 88 mm |
| Depth with packaging: | 133 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799571032 |
| Article number: | 0157.0103 |

Manufacturer: MAICO

P 1 Pole-changing switch