**Rotary switch DS 10**

Rotary switch for operating fans independently of a thermostat.

Switch for switching on and switching between controlled and continuous operation.

Switch positions: Continuous operation, Off, controlled operation.

Technical data

|  |  |
| --- | --- |
| Article: | DS 10 |
| Type of voltage: | Alternating current |
| Rated voltage: | 230 V |
| Frequency: | 50 Hz/60 Hz |
| Imax: | 16 A |
| Degree of protection: | IP 65 |
| Type of installation: | Surface-mounted |
| Weight: | 0,29 kg |
| Weight including packaging: | 0,32 kg |
| Width: | 82 mm |
| Height: | 82 mm |
| Depth: | 101 mm |
| Width with packaging: | 85 mm |
| Height with packaging: | 95 mm |
| Depth with packaging: | 135 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799574101 |
| Article number: | 0157.0410 |

Manufacturer: MAICO

DS 10 Rotary switch