**Main switch, service switch HS 3**

Service switch in accordance with VDE 0113, part 1.

Housing encapsulated in accordance with ISO.

Switch can be locked in the OFF position.

With 2 auxiliary contacts (1 N/C contact, 1 N/O contact).

HS 3: 3-pole cam-operated switch for single speed fans or for speed-controlled fans.

HS 6: 6-pole cam-operated switch for pole-changeable fans.

Technical data

|  |  |
| --- | --- |
| Article: | HS 3 |
| Type of voltage: | Three-phase AC / Alternating current |
| Rated voltage: | 230 V / 400 V |
| Maximum load: | 16 A |
| Degree of protection: | IP 65 |
| Type of installation: | Surface-mounted |
| Weight: | 0,38 kg |
| Weight including packaging: | 0,41 kg |
| Width: | 82 mm |
| Height: | 82 mm |
| Depth: | 127 mm |
| Width with packaging: | 87 mm |
| Height with packaging: | 95 mm |
| Depth with packaging: | 135 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799577362 |
| Article number: | 0157.0736 |

Manufacturer: MAICO

HS 3 Main switch, service switch