**3-step switch DS 3N**

Rotary switch for controlling 3-step ventilation units (e.g. ER 100 D exhaust air fan).

Suitable for standard recessed-mounted boxes.

With zero setting.

Technical data

|  |  |
| --- | --- |
| Article: | DS 3N |
| Rated voltage: | 230 V |
| Maximum load: | 16 A |
| Degree of protection: | IP 30 |
| Type of installation: | Recessed-mounted |
| Colour: | polar white, similar to RAL 9010, matt |
| Weight: | 0,11 kg |
| Weight including packaging: | 0,13 kg |
| Width: | 80 mm |
| Height: | 80 mm |
| Depth: | 32 mm |
| Width with packaging: | 83 mm |
| Height with packaging: | 83 mm |
| Depth with packaging: | 73 mm |
| Operating mode: | Rotary knob |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799571865 |
| Article number: | 0157.0186 |

Manufacturer: MAICO

DS 3N 3-step switch