**Motor protection switch MV 25**

Motor protection switch for fans with fitted thermal contacts.

With main contactor and control fuse.

Technical data

|  |  |
| --- | --- |
| Article: | MV 25 |
| Type of voltage: | Three-phase AC |
| Rated voltage: | 400 V |
| Frequency: | 50 Hz/60 Hz |
| Maximum load: | 25 A |
| Type of installation: | Surface-mounted |
| Weight: | 0,56 kg |
| Weight including packaging: | 0,6 kg |
| Width: | 75 mm |
| Height: | 140 mm |
| Depth: | 95 mm |
| Width with packaging: | 82 mm |
| Height with packaging: | 145 mm |
| Depth with packaging: | 96 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799577126 |
| Article number: | 0157.0712 |

Manufacturer: MAICO

MV 25 Motor protection switch