**Door contact switch TS 8**

Door contact switch, which automatically switches fans on or off if the door is closed.

Assembly on door frame and the door.

Installation instructions

Provide the required cavity for fitting on the door and door frame.

Operate the door contact switch using a low voltage (24 V) in humid areas.

Technical data

|  |  |
| --- | --- |
| Article: | TS 8 |
| Rated voltage: | 230 V |
| Maximum load: | 8 A |
| Degree of protection: | IP 50 |
| Weight: | 0,023 kg |
| Weight including packaging: | 0 kg |
| Width: | 45 mm |
| Height: | 45 mm |
| Depth: | 15 mm |
| Width with packaging: | 45 mm |
| Height with packaging: | 15 mm |
| Depth with packaging: | 45 mm |
| Packing unit: | 1 piece |
| Range: | A |
| GTIN (EAN): | 4012799571209 |
| Article number: | 0157.0120 |

Manufacturer: MAICO

TS 8 Door contact switch