**Contactor US 16 T**

Universal contactor for controlling fans and/or for loads.

Control voltage: 230 V/50 Hz, 240 V/60 Hz.

With 3 main contacts, 1 auxiliary contact (N/C contact).

Water and dust protected.

With integrated 35 mm profile rail.

Technical data

|  |  |
| --- | --- |
| Article: | US 16 T |
| Type of voltage: | Three-phase AC |
| Rated voltage: | 600 V |
| Maximum load (ohmic load): | 16 A |
| Degree of protection: | IP 55 |
| Type of installation: | Surface-mounted |
| Weight: | 0,67 kg |
| Weight including packaging: | 0,78 kg |
| Width: | 100 mm |
| Height: | 160 mm |
| Depth: | 145 mm |
| Width with packaging: | 105 mm |
| Height with packaging: | 200 mm |
| Depth with packaging: | 185 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799577690 |
| Article number: | 0157.0769 |

Manufacturer: MAICO

US 16 T Contactor