**Wall-mounted fan ETR 25**

Technical data

|  |  |
| --- | --- |
| Article: | ETR 25 |
| Air flow volume: | 900 m³/h |
| Rotating speed: | 1.380 1/min |
| Air direction: | Ventilation / Air extraction |
| Speed controllable: |  ✔  |
| Reversing capacity: |  ✔  |
| Type of voltage: | Alternating current |
| Rated voltage: | 230 V |
| Nominal output: | 32 W |
| Power consumption: | 38 W |
| Inom: | 0,16 A |
| Imax: | 0,16 A |
| Installation site: | Wall |
| Type of installation: | Surface-mounted |
| Installation position: | horizontal |
| Material: | Synthetic material |
| Colour: | Traffic white, similar to RAL 9016 |
| Weight: | 3,615 |
| Nominal size: | 250 mm |
| Sound pressure level: | 56 dB(A) |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799815051 |
| Article number: | 0081.0505 |

Manufacturer: MAICO

ETR 25 Wall-mounted fan