**Greenhouse fan EFG 25 E**

Technical data

|  |  |
| --- | --- |
| Article: | EFG 25 E |
| Air flow volume: | 570 m³/h |
| Rotating speed: | 1.360 1/min |
| Reversing capacity: | - |
| Nominal output: | 30 W |
| Power consumption: | 30 W |
| Inom: | 0,24 A |
| Imax: | 0,24 A |
| Degree of protection: | IP X4 |
| Weight: | 5,93 |
| Nominal size: | 250 mm |
| Airstream temperature at nominal current: | 60 °C |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799814023 |
| Article number: | 0081.0402 |

Manufacturer: MAICO

EFG 25 E Greenhouse fan