**Greenhouse fan EFG 30 E**

Technical data

|  |  |
| --- | --- |
| Article: | EFG 30 E |
| Air flow volume: | 800 m³/h |
| Rotating speed: | 1.340 1/min |
| Reversing capacity: |  -  |
| Nominal output: | 35 W |
| Power consumption: | 35 W |
| Inom: | 0,25 A |
| Imax: | 0,25 A |
| Degree of protection: | IP X4 |
| Weight: | 6,915 |
| Nominal size: | 300 mm |
| Airstream temperature at nominal current: | 60 °C |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799814030 |
| Article number: | 0081.0403 |

Manufacturer: MAICO

EFG 30 E Greenhouse fan