**Greenhouse fan EFG 40 D**

Technical data

|  |  |
| --- | --- |
| Article: | EFG 40 D |
| Air flow volume: | 1.800 m³/h |
| Rotating speed: | 1.300 1/min |
| Reversing capacity: | ✔ |
| Nominal output: | 50 W |
| Power consumption: | 50 W |
| Inom: | 0,25 A |
| Imax: | 0,3 A |
| Degree of protection: | IP X4 |
| Weight: | 9,95 |
| Nominal size: | 400 mm |
| Airstream temperature at nominal current: | 55 °C |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799814078 |
| Article number: | 0081.0407 |

Manufacturer: MAICO

EFG 40 D Greenhouse fan