**Centrifugal roof fan DRD 50/8**

Technical data

|  |  |
| --- | --- |
| Article: | DRD 50/8 |
| Air flow volume: | 6.300 m³/h |
| Rotating speed: | 715 1/min |
| Nominal output: | 640 W |
| Inom: | 1,5 A |
| Imax: | 1,7 A |
| Pole-changeable: | - |
| Installation site: | Roof |
| Installation position: | vertical |
| Material: | Sheet steel, galvanised |
| Weight: | 124 |
| Airstream temperature at nominal current: | 60 °C |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799871163 |
| Article number: | 0087.0116 |

Manufacturer: MAICO

DRD 50/8 Centrifugal roof fan