**Centrifugal roof fan DRD 50/6**

Technical data

|  |  |
| --- | --- |
| Article: | DRD 50/6 |
| Air flow volume: | 8.300 m³/h |
| Rotating speed: | 930 1/min |
| Nominal output: | 1.260 W |
| Inom: | 2,6 A |
| Imax: | 3,3 A |
| Pole-changeable: | - |
| Installation site: | Roof |
| Installation position: | vertical |
| Material: | Sheet steel, galvanised |
| Weight: | 124 |
| Airstream temperature at nominal current: | 60 °C |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799871132 |
| Article number: | 0087.0113 |

Manufacturer: MAICO

DRD 50/6 Centrifugal roof fan