**Centrifugal roof fan DRD 63/86**

Technical data

|  |  |
| --- | --- |
| Article: | DRD 63/86 |
| Air flow volume: | 14.000 m³/h / 18.500 m³/h |
| Rotating speed: | 715 1/min / 930 1/min |
| Nominal output: | 2.000 W / 4.000 W |
| Inom: | 4 A / 8 A |
| Imax: | 4 A / 8,3 A |
| Pole-changeable: | ✔ |
| Number of poles at high speed: | 6 |
| Number of poles at low speed: | 8 |
| Installation site: | Roof |
| Installation position: | vertical |
| Material: | Sheet steel, galvanised |
| Weight: | 225 |
| Airstream temperature at nominal current: | 60 °C |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799871590 |
| Article number: | 0087.0159 |

Manufacturer: MAICO

DRD 63/86 Centrifugal roof fan