**Axial duct fan DZR 35/2 A-Ex**

Technical data

|  |  |
| --- | --- |
| Article: | DZR 35/2 A-Ex |
| Air flow volume: | 6.000 m³/h |
| Rotating speed: | 2.750 1/min |
| Nominal output: | 900 W |
| Inom: | 1,81 A |
| Imax: | 1,92 A |
| Weight: | 20,7 |
| IA/IN: | 5,7 |
| Certified as explosion proof: | 84/3893 |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799867722 |
| Article number: | 0086.0772 |

Manufacturer: MAICO

DZR 35/2 A-Ex Axial duct fan