**Internal grille MLG 30**

Internal grille for ventilation and air extraction.

Technical data

|  |  |
| --- | --- |
| Article: | MLG 30 |
| Air direction: | Ventilation / Air extraction |
| Max. flow velocity: | 2 m/s |
| Installation site: | Wall |
| Material: | Sheet steel |
| Housing material: | Sheet steel, stove-enamelled |
| Colour: | White |
| Weight: | 1,4 |
| Suitable for nominal size: | 300 mm |
| Open cross section: | 520 cm² |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799510635 |
| Article number: | 0151.0063 |

Manufacturer: MAICO

MLG 30 Internal grille