**Outside air opening ALD 160 VA**

Outside air opening for draught-free, decentralised domestic ventilation.

Type of shutter: Manual (0% or 100% position).

Very good insulation.

Flat, visually appealing design.

Good air distribution.

No electrical connection required.

ALD 160 packing unit: Inner part made of plastic, dust filter

ISO Coarse 30 % (G2), wall sleeve up to 500 mm with storm protection and sound insulation, manual shutter, rectangular plastic external grille including fly screen.

ALD 160 VA packing unit: Inner part made of plastic, dust filter

ISO Coarse 30 % (G2), wall sleeve up to 500 mm with storm protection and sound insulation, manual shutter, round stainless external grille including fly screen.

Accessories: ALDF 125/160 G2 or ALDF 125/160 G3 replacement filter.

Technical data

|  |  |
| --- | --- |
| Article: | ALD 160 VA |
| Air direction: | Ventilation |
| Max. volumetric flow: | 30 m³/h |
| Installation site: | Wall |
| Grille material: | Synthetic (internal grille) / Stainless steel (external grille) |
| Housing material: | Synthetic material |
| Colour: | Pure white, similar to RAL 9010 |
| Weight: | 1,47 kg |
| Weight including packaging: | 1,79 kg |
| Type of filter: | Dust filter |
| Filter class: | ISO Coarse 30 % (G2) |
| Type of shutter: | manual, can be locked |
| Nominal size: | 160 mm |
| Width: | 175 mm |
| Height: | 175 mm |
| Depth: | 572,5 mm |
| Width with packaging: | 190 mm |
| Height with packaging: | 190 mm |
| Depth with packaging: | 585 mm |
| Ambient temperature: | 60 °C |
| Rated max. element normal difference in noise level Dn,w: | 53 dB |
| Packing unit: | 1 piece |
| Range: | B |
| GTIN (EAN): | 4012799520702 |
| Article number: | 0152.0070 |

Manufacturer: MAICO

ALD 160 VA Outside air opening