**Air distributor box made of sheet metal, 12-way MF-BV75-160-12**

Air distributor box made of sheet metal with sound-insulated inner coating.

Front sheet metal plate fitted with MF-WE integrated plastic slide-in adaptors for accurate and rapid insertion of MF-F flexible steel ducts.

Upon delivery, half of the slide-in adaptors are fitted with shutters.

Equipped with 4 rubber fixing brackets for sound-insulated wall / ceiling mounting.

3 removable revision connection plates (2 x at side, 1 at bottom on distributor box).

Main duct connection at face end (NW 125/NW 160) can be moved onto revision connection plates.

Use as straight or 90° distributor.

Accessories needed: MF-FDR gaskets

Technical data

|  |  |
| --- | --- |
| Article: | MF-BV75-160-12 |
| Air direction: | Ventilation or air extraction |
| Volumetric flow: | 360 m³/h recommended |
| Material: | Sheet steel, galvanised |
| Weight: | 11,18 kg |
| Weight including packaging: | 13,12 kg |
| Connection diameter: | 160 mm |
| Flexible steel duct connection diameter: | 75 mm |
| Number of couplings: | 12 |
| Width: | 650 mm |
| Height: | 200 mm |
| Depth: | 500 mm |
| Width with packaging: | 670 mm |
| Height with packaging: | 225 mm |
| Depth with packaging: | 540 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799185284 |
| Article number: | 0018.0528 |

Manufacturer: MAICO

MF-BV75-160-12 Air distributor box made of sheet metal, 12-way