**Sound insulation set KSD-D**

4 rubber damping elements with galvanised shim for structure-borne sound-insulated ceiling mounting of ESR -2 EC ventilation boxes in accordance with DIN 4109.

Other mounting material such as threaded rods, nuts etc. are not included in the scope of supply.

Technical data

|  |  |
| --- | --- |
| Article: | KSD-D |
| Material: | Thermoplastic elastomer (TPE) |
| Colour: | Black |
| Weight: | 0,03 kg |
| Weight including packaging: | 0,04 kg |
| Fire protection: | Fire class B2 according to DIN 4102, non-dripping |
| Width: | 80 mm |
| Height: | 50 mm |
| Depth: | 50 mm |
| Width with packaging: | 80 mm |
| Height with packaging: | 30 mm |
| Depth with packaging: | 50 mm |
| Thread: | M8 |
| Ambient temperature: | -50 °C up to 110 °C |
| Packing unit: | 4 pieces |
| Range: | C |
| GTIN (EAN): | 4012799925217 |
| Article number: | 0092.0521 |

Manufacturer: MAICO

KSD-D Sound insulation set