**Differential pressure transmitter DS 500**

Pressure transmitter in plastic housing for use in air and non-aggressive gases.

Output signal of between 0-10 V (upon delivery) and 4-20 mA can be selected.

Activation time can also be selected: 1 s (upon delivery) or 100 ms.

Scope of delivery:

1 x pressure transmitter

2 x plastic pressure probes

1 x 2 m PVC hose

Technical data

|  |  |
| --- | --- |
| Article: | DS 500 |
| Max. excess pressure: | 20 kPa |
| Operating range: | 0 - 500 Pa / 0 - 1000 Pa |
| Type of voltage: | Direct current |
| Rated voltage: | 18 V - 30 V DC |
| Output signal: | 0 V - 10 V |
| Degree of protection: | IP 54 |
| Weight: | 0,17 kg |
| Weight including packaging: | 0,21 kg |
| Width: | 130 mm |
| Height: | 130 mm |
| Depth: | 56 mm |
| Width with packaging: | 140 mm |
| Height with packaging: | 75 mm |
| Depth with packaging: | 115 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799571186 |
| Article number: | 0157.0118 |

Manufacturer: MAICO

DS 500 Differential pressure transmitter