**Outside air opening ZE 45 F white**

Sound insulated outside air opening for decentralised domestic ventilation.

Linear control of the air flow.

For installation in window frames.

Wooden window: Slots are necessary in the window frame.

Aluminium and PVC windows: A ZEK 45 F air channel is necessary for hollow chamber profiles.

The volumetric flow is approx. 22 m3 /h with 10 Pa pressure difference and a fully opened valve.

Packing unit: Internal part, dust or insect filter, weather protection grille with fly screen.

Accessories: ZEK 45 F flat channel, ZE 45 GF flat grille, ZEF replacement filter.

Technical data

|  |  |
| --- | --- |
| Article: | ZE 45 F white |
| Air direction: | Ventilation |
| Installation site: | Window |
| Material: | Aluminium |
| Colour: | Traffic white, similar to RAL 9016 |
| Weight: | 0,8 kg |
| Weight including packaging: | 0,83 kg |
| Type of filter: | Dust filter |
| Filter class: | G2 |
| Type of shutter: | manual |
| Width: | 450 mm |
| Height: | 30 mm |
| Depth: | 100 mm |
| Width with packaging: | 485 mm |
| Height with packaging: | 40 mm |
| Depth with packaging: | 135 mm |
| Ambient temperature: | 60 °C |
| Rated max. element normal difference in noise level Dn,w: | 40 dB |
| Sound insulation: | yes |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799520443 |
| Article number: | 0152.0044 |

Manufacturer: MAICO

ZE 45 F white Outside air opening