**Internal grille, adjustable AZE 100 P**

Hygiene grille for ventilation and air extraction.

Alternative to the disk valve.

Minimum pressure loss.

Covered filter keeps the duct clean.

AZE 100 P: can be washed.

Linear air flow control via internal valve disk.

Can be set quickly, easily and precisely.

Setting can be permanently fixed.

High-quality design for the domestic area.

Cover can be removed without tools for cleaning.

Sealing tape included in the scope of delivery.

AZE 100 accessories: ZRF.. spare air filter.

AZE 100 P accessories: AZP replacement air filter.

Technical data

|  |  |
| --- | --- |
| Article: | AZE 100 P |
| Air direction: | Ventilation and air extraction |
| Installation: | Inside |
| Installation site: | Wall |
| Type of installation: | Surface-mounted |
| Material: | Synthetic material |
| Colour: | Traffic white, similar to RAL 9016 |
| Weight: | 0,2 kg |
| Weight including packaging: | 0,166 kg |
| Filter class: | PPI 20 |
| Suitable for nominal size: | 100 mm |
| Width: | 150 mm |
| Height: | 150 mm |
| Depth: | 51,5 mm |
| Width with packaging: | 150 mm |
| Height with packaging: | 50 mm |
| Depth with packaging: | 150 mm |
| Ambient temperature: | 60 °C |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799599623 |
| Article number: | 0059.0962 |

Manufacturer: MAICO

AZE 100 P Internal grille, adjustable