**Sound-insulated ventilation box ESR 12-3 EC**

Technical data

|  |  |
| --- | --- |
| Article: | ESR 12-3 EC |
| Air flow volume: | 490 m³/h |
| Rotating speed: | 4.010 1/min |
| Impeller type: | radial |
| Speed controllable: |  ✔  |
| Rated voltage: | 230 V |
| Frequency: | 50 Hz/60 Hz |
| Nominal output: | 121 W |
| Imax: | 1 A |
| Degree of protection: | IP 54 |
| Insulation class: | F |
| Installation site: | Wall / ceiling |
| Installation position: | vertical / horizontal |
| Material: | Sheet steel, galvanised |
| Colour: | Silver |
| Weight: | 12,32 kg |
| Weight including packaging: | 13,63 kg |
| Swivelling fan: |  ✔  |
| Nominal size: | 125 mm |
| Width: | 386 mm |
| Height: | 232 mm |
| Depth: | 485 mm |
| Width with packaging: | 395 mm |
| Height with packaging: | 275 mm |
| Depth with packaging: | 565 mm |
| Airstream temperature at IMax: | 50 °C |
| Ambient temperature: | -30 °C up to 50 °C |
| Packing unit: | 1 piece |
| Range: | E |
| GTIN (EAN): | 4012799981039 |
| Article number: | 0080.1000 |

Manufacturer: MAICO

ESR 12-3 EC Sound-insulated ventilation box