**Disk valve, stainless steel TM-V2A 12**

Stainless steel disk valves for ventilation and air extraction with connection socket.

With loose installation ring and spring clamp for simple installation.

Linear air flow control via rotatable valve disk.

Recommended accessories: FFE grease filter element for use in rooms where the exhaust air contains grease (e.g. kitchens etc.).

Technical data

|  |  |
| --- | --- |
| Article: | TM-V2A 12 |
| Air direction: | Ventilation and air extraction |
| Volumetric flow: | 40 m³/h / 60 m³/h / 80 m³/h / 130 m³/h at 11 Pa / 23 Pa / 51 Pa / 139 Pa |
| Material: | Stainless steel |
| Colour: | Stainless steel, brushed |
| Weight: | 0,27 kg |
| Weight including packaging: | 0,28 kg |
| Suitable for nominal size: | 125 mm |
| Width: | 170 mm |
| Height: | 170 mm |
| Depth: | 52 mm |
| Width with packaging: | 175 mm |
| Height with packaging: | 175 mm |
| Depth with packaging: | 60 mm |
| Sound power level: | 35 dB(A) / at max. 130 m³/h |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799513759 |
| Article number: | 0151.0375 |

Manufacturer: MAICO

TM-V2A 12 Disk valve, stainless steel