**Sound-insulated ventilation box ESR 25/1**

Technical data

|  |  |
| --- | --- |
| Article: | ESR 25/1 |
| Air flow volume: | 1.100 m³/h |
| Rotating speed: | 1.840 1/min |
| Speed controllable: |  -  |
| Nominal output: | 280 W |
| Inom: | 0,9 A |
| Imax: | 1,3 A |
| Degree of protection: | IP X4 |
| Insulation class: | F |
| Weight: | 18,3 |
| Nominal size: | 250 mm |
| Airstream temperature at nominal current: | 60 °C |
| Airstream temperature at IMax: | 60 °C |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799802846 |
| Article number: | 0080.0284 |

Manufacturer: MAICO

ESR 25/1 Sound-insulated ventilation box