**Fire protection ceiling barrier TS 18 DN 140**

Fire protection ceiling barrier for ER exhaust air systems.

With continuous open cross-section and smooth inner surfaces.

General official approval, approval number Z-41.3-556.

Certificate of approval at www.maico-fans.com.

Fire resistance class K90-18017.

Maintenance-free.

Technical data

|  |  |
| --- | --- |
| Article: | TS 18 DN 140 |
| Air direction: | Ventilation and air extraction |
| Installation site: | Ceiling |
| Type of installation: | Recessed-mounted |
| Material: | Sheet steel |
| Weight: | 1,37 kg |
| Weight including packaging: | 1,42 kg |
| Fire protection: | yes |
| Suitable for nominal size: | 140 mm |
| Width: | 273 mm |
| Height: | 167 mm |
| Depth: | 173 mm |
| Width with packaging: | 274 mm |
| Height with packaging: | 168 mm |
| Depth with packaging: | 174 mm |
| Approval number: | Z-41.3-556 |
| Packing unit: | 1 piece |
| Range: | B |
| GTIN (EAN): | 4012799513223 |
| Article number: | 0151.0322 |

Manufacturer: MAICO

TS 18 DN 140 Fire protection ceiling barrier