**Outside air wall connection KW-AL 20E**

The attractive stainless steel outside air wall supports are fitted on the outside wall of a building and are intended for outside air intake.

The outside air is drawn in at the bottom.

An outside air cowl with bird protection grille is included in the scope of delivery.

Technical data

|  |  |
| --- | --- |
| Article: | KW-AL 20E |
| Air direction: | Ventilation |
| Installation site: | Outside wall |
| Material: | Stainless steel (V2A) |
| Colour: | Stainless steel, brushed |
| Weight: | 1,4 kg |
| Weight including packaging: | 1,62 kg |
| Nominal size: | 200 mm |
| Width: | 280 mm |
| Height: | 292 mm |
| Depth: | 126 mm |
| Width with packaging: | 320 mm |
| Height with packaging: | 300 mm |
| Depth with packaging: | 150 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799520818 |
| Article number: | 0152.0081 |

Manufacturer: MAICO

KW-AL 20E Outside air wall connection