**Centrifugal roof fan DRD 31 EC**

Features

Low energy consumption thanks to EC technology.

Attractive aluminium housing.

Easily detachable cover.

Galvanised protective grille on the discharge side with protection against accidental contact.

Sturdy eyebolts enable transport by crane.

Impeller with plastic blades curved to the rear, dynamically balanced at two levels, in accordance with performance level 6.3, DIN ISO 1940.

Motor

DC motor.

Rated voltage 230 V, 50 Hz.

Thermal overload protection as a standard feature.

Speed output.

0 - 10 V DC control input

Soft start.

IP X4 degree of protection with closed housing cover.

Electrical connection

In terminal box, easily accessible once housing cover has been removed.

Security instructions

The fan can be operated only if the protection against accidental contact with the impeller is guaranteed for fans with a free inlet.

Technical data

|  |  |
| --- | --- |
| Article: | DRD 31 EC |
| Air flow volume: | 3.500 m³/h |
| Rotating speed: | 1.570 1/min |
| Impeller type: | radial |
| Speed controllable: | ✔ |
| Reversing capacity: | - |
| Type of voltage: | Alternating current |
| Rated voltage: | 230 V |
| Frequency: | 50 Hz |
| Nominal output: | 370 W |
| Imax: | 1,65 A |
| Degree of protection: | IP 54 |
| Installation site: | Roof |
| Installation position: | vertical |
| Material: | Aluminium |
| Weight: | 15,77 kg |
| Weight including packaging: | 20,02 kg |
| Nominal size: | 315 mm |
| Width: | 630 mm |
| Height: | 400 mm |
| Depth: | 630 mm |
| Width with packaging: | 715 mm |
| Height with packaging: | 530 mm |
| Depth with packaging: | 715 mm |
| Airstream temperature at IMax: | -25 °C up to 60 °C |
| Packing unit: | 1 piece |
| Range: | E |
| GTIN (EAN): | 4012799871729 |
| Article number: | 0087.0172 |

Manufacturer: MAICO

DRD 31 EC Centrifugal roof fan