**Reversing switch, pole-changing switch WP 1**

Pole-changing switch for controlling pole-changeable fans.

Step switch for 2 speeds.

Technical data

|  |  |
| --- | --- |
| Article: | WP 1 |
| Air direction: | Ventilation and air extraction |
| Type of voltage: | Three-phase AC |
| Rated voltage: | 500 V |
| Maximum load: | 16 A |
| Degree of protection: | IP 65 |
| Motor: | Dahlander circuit |
| Type of installation: | Surface-mounted |
| Weight: | 0,42 kg |
| Weight including packaging: | 0,45 kg |
| Width: | 82 mm |
| Height: | 82 mm |
| Depth: | 127 mm |
| Width with packaging: | 87 mm |
| Height with packaging: | 93 mm |
| Depth with packaging: | 133 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799571056 |
| Article number: | 0157.0105 |

Manufacturer: MAICO

WP 1 Reversing switch, pole-changing switch