**Temperature sensor NTC 15**

Temperature sensor with grommet for switching off the unit at a supply air temperature below 10 °C when using a warm water register.

This is claimed by the Passivhausinstitut for the protection of an ideal warm water register, e.g. WRH 12-1, in the supply air.

Accessories for ventilation unit with heat recovery WS 170.

Technical data

|  |  |
| --- | --- |
| Article: | NTC 15 |
| Weight: | 0,05 kg |
| Weight including packaging: | 0,05 kg |
| Width: | 200 mm |
| Height: | 80 mm |
| Depth: | 100 mm |
| Width with packaging: | 200 mm |
| Height with packaging: | 20 mm |
| Depth with packaging: | 100 mm |
| Packing unit: | 1 piece |
| Suitable for products: | WS 170... |
| Range: | K |
| GTIN (EAN): | 4012799578338 |
| Article number: | 0157.0833 |

Manufacturer: MAICO

NTC 15 Temperature sensor