**Shutter AP 100**

Airstream-operated shutters for air extraction.

Exterior wall connection when using WH wall sleeve.

With covered screw holes.

Sealing strip included in the scope of delivery.

Accessories: FG fly screen can be used.

Technical data

|  |  |
| --- | --- |
| Article: | AP 100 |
| Air direction: | Air extraction |
| Loss of pressure: | 10 Pa |
| Installation site: | Wall |
| Material: | Synthetic material, weather and UV resistant |
| Colour: | Traffic white, similar to RAL 9016 |
| Weight: | 0,11 kg |
| Weight including packaging: | 0,12 kg |
| Type of shutter: | Airstream-operated opening/closing |
| Suitable for nominal size: | 100 mm |
| Width: | 150 mm |
| Height: | 150 mm |
| Depth: | 50 mm |
| Width with packaging: | 151 mm |
| Height with packaging: | 151 mm |
| Depth with packaging: | 51 mm |
| Ambient temperature: | 60 °C |
| Packing unit: | 1 piece |
| Range: | A |
| GTIN (EAN): | 4012799990055 |
| Article number: | 0059.1058 |

Manufacturer: MAICO

AP 100 Shutter