**Room air control RLS T1 WS**

Graphic colour TFT display ("touch screen") with user-friendly intuitive menu structure.

Optional as accessories for Trio, WS 160 Flat, WS 170, WR 310/WR 410, WS 320 and WS 470 centralised ventilation units.

Setting time programs, operating modes, ventilation levels, temperatures etc.

Amongst other things includes integrated NTC room temperature sensor, mini USB port and 4-wire bus connection (RS 485 includes power supply).

Display resolution: 480 x 272 pixels (screen diagonal 4.3").

Technical data

|  |  |
| --- | --- |
| Article: | RLS T1 WS |
| Type of voltage: | Alternating current |
| Rated voltage: | 12 V DC |
| Type of installation: | Surface-mounted |
| Material: | Synthetic material |
| Synthetic material definition: | PVC-free polystyrene |
| Colour: | white |
| Weight: | 0,21 kg |
| Weight including packaging: | 0,3 kg |
| Width: | 127 mm |
| Height: | 93 mm |
| Depth: | 50 mm |
| Width with packaging: | 165 mm |
| Height with packaging: | 180 mm |
| Depth with packaging: | 51 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799578352 |
| Article number: | 0157.0835 |

Manufacturer: MAICO

RLS T1 WS Room air control