**Combi sensor WS 75 VOC**

The combi sensor has three sensors: Temperature, humidity and VOC.

The ventilation unit is controlled according to the measured humidity values and the volatile organic compounds present.

Technical data

|  |  |
| --- | --- |
| Article: | WS 75 VOC |
| Material: | Synthetic material |
| Colour: | green |
| Weight: | 0,01 kg |
| Weight including packaging: | 0,02 kg |
| Width: | 63 mm |
| Height: | 25 mm |
| Depth: | 16 mm |
| Width with packaging: | 90 mm |
| Height with packaging: | 85 mm |
| Depth with packaging: | 45 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799992493 |
| Article number: | 0157.1591 |

Manufacturer: MAICO

WS 75 VOC Combi sensor