**Combi-wall connections Duo KWS W**

Stainless steel external cover with separate outside and outgoing air flow. Air outlet at front, air intake from below.

Scope of delivery:

Base plate

Protective cover

Technical data

|  |  |
| --- | --- |
| Article: | Duo KWS W |
| Installation site: | Outside wall |
| Type of installation: | Surface-mounted |
| Material: | Stainless steel |
| Colour: | White powder-coated, similar to RAL 9010 |
| Weight: | 1,54 kg |
| Weight including packaging: | 1,81 kg |
| Connection diameter: | 125 mm |
| Width: | 378 mm |
| Height: | 179 mm |
| Depth: | 93 mm |
| Width with packaging: | 395 mm |
| Height with packaging: | 250 mm |
| Depth with packaging: | 160 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799990956 |
| Article number: | 0093.1441 |

Manufacturer: MAICO

Duo KWS W Combi-wall connections