**Radio switch XS 1**

Radio switch for location-independent switching of AC fans or other consumers, such as light, circulation pump, etc.

For redevelopments and retrofit installations. No painting or wallpapering.

Tiles don't need to be removed or renewed.

Application wherever no control cable can be installed.

Radio switch can be used on the move.

Radio switch can be screwed on or attached to a glass surface.

Simple transmitter teaching-in saves on time-consuming programming.

Batteries included in scope of delivery.

Radio system consists of XS 1 radio switch and at least one XE 1 radio receiver.

Technical data

|  |  |
| --- | --- |
| Article: | XS 1 |
| Battery: | 2 x 3 V |
| Mains cable: | not required |
| Type of installation: | Surface-mounted |
| Colour: | Pure white, similar to RAL 9010 |
| Weight: | 0,1 kg |
| Weight including packaging: | 0,14 kg |
| Width: | 88 mm |
| Height: | 88 mm |
| Depth: | 32 mm |
| Width with packaging: | 103 mm |
| Height with packaging: | 89 mm |
| Depth with packaging: | 85 mm |
| Radio frequency: | 433 MHz |
| Number of radio channels: | 1 Channel |
| Transmission range in the clear area: | 100 m |
| Transmission range in the building: | 30 m |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799573449 |
| Article number: | 0157.0344 |

Manufacturer: MAICO

XS 1 Radio switch