**Differential pressure controller DW 1000**

Differential pressure controller for monitoring filter, fan and system pressure in ventilation systems.

Switchover contact for switched current max. 5 A, 250 V AC and 0.8 A for inductive loads or 2 A, 30 V DC.

Setpoint range: 100 Pa to 1000 Pa.

Media: Air and non-aggressive gas.

Electrical connection with PG 11 cable screw-connections and screw terminals.

Packing unit: Pressure switch with hose couplings, adjustable scale in mbar, installation bracket, 2 m hose connection set.

Accessories for TFE and TFP air filters.

Safety instructions

Prevent condensation and ice forming on the differential pressure controller.

Technical data

|  |  |
| --- | --- |
| Article: | DW 1000 |
| Degree of protection: | IP 54 |
| Installation position: | vertical |
| Weight: | 0,19 kg |
| Weight including packaging: | 0,24 kg |
| Width: | 125 mm |
| Height: | 103 mm |
| Depth: | 89,4 mm |
| Width with packaging: | 126 mm |
| Height with packaging: | 104 mm |
| Depth with packaging: | 100 mm |
| Ambient temperature: | 85 °C |
| Packing unit: | 1 piece |
| Range: | D |
| GTIN (EAN): | 4012799577522 |
| Article number: | 0157.0752 |

Manufacturer: MAICO

DW 1000 Differential pressure controller