**shell installation kit WS 75 RSUP**

Shell installation kit for installation in the exterior wall for ventilation unit with WS 75 Powerbox H heat recovery for a wall thickness of up to 500 mm.

Scope of delivery:

Installation box (width x height x depth: 534 x 1066 x 152 mm) with integrated drilling template

Two wall sleeves (outer Ø 125 mm, inner Ø 90 mm, length 500 mm) made from EPP, each with two plaster protective covers

Two WS 75 A sheet metal adapters, each with two connections for the MF-M75 flexible duct, plus one plug per adapter

Technical data

|  |  |
| --- | --- |
| Article: | WS 75 RSUP |
| Housing material: | Sheet steel, powder coated |
| Colour: | Traffic black, RAL 9017 |
| Weight: | 9,77 kg |
| Weight including packaging: | 11,96 kg |
| Width: | 534 mm |
| Height: | 1.066 mm |
| Depth: | 152 mm |
| Width with packaging: | 595 mm |
| Height with packaging: | 1.130 mm |
| Depth with packaging: | 210 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799992547 |
| Article number: | 0093.1616 |

Manufacturer: MAICO

WS 75 RSUP shell installation kit