**Room air control RLS 1 WR**

Included in scope of supply of WS 120 Trio, WS 160 Flat, WS 170, WS 300 Flat, WR 310 / WR 410, WS 320 and WS 470 ventilation units.

Other control units can be connected in parallel.

4 ventilation levels can be set using buttons.

With LED-based filter change message.

With LED-based fault indication.

Included in scope of supply for adapter plate for recessed-mounted box.

Control cable for LiYY 7x0.34 mm² units.

Voltage supply by WS / WR units.

Technical data

|  |  |
| --- | --- |
| Article: | RLS 1 WR |
| Type of voltage: | Alternating current |
| Rated voltage: | 12 V |
| Material: | Synthetic material |
| Synthetic material definition: | PVC-free polystyrene |
| Weight: | 0,09 kg |
| Weight including packaging: | 0,1 kg |
| Width: | 80 mm |
| Height: | 80 mm |
| Depth: | 35 mm |
| Width with packaging: | 87 mm |
| Height with packaging: | 87 mm |
| Depth with packaging: | 45 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799578093 |
| Article number: | 0157.0809 |

Manufacturer: MAICO

RLS 1 WR Room air control