**Outside air wall connection KW-AL 16E**

The attractive stainless steel outside air wall supports are fitted on the outside wall of a building and are intended for outside air intake.

The outside air is drawn in at the bottom.

An outside air cowl with bird protection grille is included in the scope of delivery.

Technical data

|  |  |
| --- | --- |
| Article: | KW-AL 16E |
| Air direction: | Ventilation |
| Installation site: | Outside wall |
| Material: | Stainless steel (V2A) |
| Colour: | Stainless steel, brushed |
| Weight: | 0,9 kg |
| Weight including packaging: | 1,03 kg |
| Nominal size: | 160 mm |
| Width: | 228 mm |
| Height: | 232 mm |
| Depth: | 100 mm |
| Width with packaging: | 250 mm |
| Height with packaging: | 250 mm |
| Depth with packaging: | 110 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799520771 |
| Article number: | 0152.0077 |

Manufacturer: MAICO

KW-AL 16E Outside air wall connection