**Air filter TFE 35-4**

Air filter for ventilation systems.

Inspection lid can be removed for easy filter exchange.

With filter insert made of synthetic fibre.

Filter insert cannot be regenerated.

With rubber seal on the air connection couplings.

Accessories: Replacement air filter FE.. .

Recommended accessories: DW 1000 differential pressure controller.

Installation instructions

Monitor filter resistance using DW 1000 differential pressure controller.

Technical data

|  |  |
| --- | --- |
| Article: | TFE 35-4 |
| Installation position: | vertical / horizontal |
| Housing material: | Sheet steel, galvanised |
| Weight: | 12,11 kg |
| Weight including packaging: | 12,99 kg |
| Filter class: | ISO Coarse 70 % (G4) |
| Nominal size: | 355 mm |
| Width: | 505 mm |
| Height: | 495 mm |
| Depth: | 550 mm |
| Width with packaging: | 510 mm |
| Height with packaging: | 550 mm |
| Depth with packaging: | 610 mm |
| Ambient temperature: | 100 °C |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799490814 |
| Article number: | 0149.0081 |

Manufacturer: MAICO

TFE 35-4 Air filter