**Shutter, pull device VD 50**

Airstream operated shutters with pull device for manual operation.

Can be used only in rooms up to 5 m high due to thermal convection.

For vertical air directions and air extraction only.

Technical data

|  |  |
| --- | --- |
| Article: | VD 50 |
| Air direction: | Air extraction |
| Material: | Sheet steel |
| Weight: | 6,8 kg |
| Weight including packaging: | 6,84 kg |
| Type of shutter: | Airstream-operated opening/closing |
| Suitable for nominal size: | 500 mm |
| Width with packaging: | 570 mm |
| Height with packaging: | 420 mm |
| Depth with packaging: | 570 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799931065 |
| Article number: | 0093.0106 |

Manufacturer: MAICO

VD 50 Shutter, pull device