**Roof socket for corrugated and trapezoidal roofs SOWT 50**

Pitched roof socket for assembly of roof fans.

With sound and heat insulation made of abrasion-resistant and non-flammable mineral fibre plates.

Standard models for up to 30° roof pitch.

Varying socket heights and models for roof pitches of more than 30° are possible on request.

For use on trapezoidal and corrugated roofs.

Matching profile shape must be prepared by the customer.

Profile sheet metal must be provided by the customer.

Note: Corrugated and trapezoidal roof sockets are produced to the customer's specifications. Therefore they cannot be returned.

Technical data

|  |  |
| --- | --- |
| Article: | SOWT 50 |
| Model: | roof incline of up to 30° |
| Housing material: | Sheet steel, galvanised |
| Weight: | 26 kg |
| Weight including packaging: | 27 kg |
| Suitable for nominal size: | 500 mm |
| Width: | 1.145 mm |
| Height: | 290 mm |
| Depth: | 1.145 mm |
| Width with packaging: | 1.200 mm |
| Height with packaging: | 1.150 mm |
| Depth with packaging: | 620 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799990383 |
| Article number: | 0093.1032 |

Manufacturer: MAICO

SOWT 50 Roof socket for corrugated and trapezoidal roofs