**Sound-insulated ventilation box ESR 16/1**

Technical data

|  |  |
| --- | --- |
| Article: | ESR 16/1 |
| Air flow volume: | 380 m³/h |
| Rotating speed: | 2.000 1/min |
| Speed controllable: | - |
| Nominal output: | 85 W |
| Inom: | 0,4 A |
| Imax: | 0,4 A |
| Degree of protection: | IP X4 |
| Insulation class: | B |
| Weight: | 12,6 |
| Nominal size: | 160 mm |
| Airstream temperature at nominal current: | 55 °C |
| Airstream temperature at IMax: | 55 °C |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799802822 |
| Article number: | 0080.0282 |

Manufacturer: MAICO

ESR 16/1 Sound-insulated ventilation box