**Motor protection switch MVE 10**

Motor protection switch for fans with fitted thermal contacts.

With main contactor and control fuse.

Technical data

|  |  |
| --- | --- |
| Article: | MVE 10 |
| Type of voltage: | Alternating current |
| Rated voltage: | 230 V |
| Frequency: | 50 Hz/60 Hz |
| Maximum load: | 10 A |
| Minimum load: | 0,4 A |
| Type of installation: | Surface-mounted |
| Weight: | 0,5 kg |
| Weight including packaging: | 0,53 kg |
| Width: | 75 mm |
| Height: | 140 mm |
| Depth: | 95 mm |
| Width with packaging: | 82 mm |
| Height with packaging: | 145 mm |
| Depth with packaging: | 96 mm |
| Packing unit: | 1 piece |
| Range: | D |
| GTIN (EAN): | 4012799577119 |
| Article number: | 0157.0711 |

Manufacturer: MAICO

MVE 10 Motor protection switch