**Room air control RLS PP-K1**

The room air control is needed as an accessory for PushPull 60 KA and PushPull 60 KL.

Room air control RLS PP-K1 features the following setting options:

Continuous ventilation (with heat recovery), cross-ventilation and dehumidification operating modes.

5 ventilation levels between 17 and 55 m³/h.

No "Off" system level.

Up to 6 units can be controlled at the same time through an RLS PP-K room air control.

Technical data

|  |  |
| --- | --- |
| Article: | RLS PP-K1 |
| Type of voltage: | Alternating current |
| Rated voltage: | 230 V |
| Degree of protection: | IP X0 |
| Mains cable: | 3 x 1,5 mm² |
| Installation site: | Wall |
| Type of installation: | Recessed-mounted |
| Installation position: | vertical |
| Weight: | 0,27 kg |
| Weight including packaging: | 0,45 kg |
| Width: | 80 mm |
| Height: | 150 mm |
| Depth: | 65 mm |
| Width with packaging: | 200 mm |
| Height with packaging: | 165 mm |
| Depth with packaging: | 143 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799571933 |
| Article number: | 0157.0193 |

Manufacturer: MAICO

RLS PP-K1 Room air control