**Air purifier CleanBox 300**

Features

Filters 99.995 % of the bacteria and viruses out of the air.

ISO ePM1 ≥ 50 % (F7) full filter + HEPA H14 filter.

Modern, timeless design.

Can be set steplessly.

Quiet and draught-free operation.

Robust and safe housing made of sheet steel.

Energy-saving EC fan.

Plug & Play via socket.

Mobile application range thanks to transport rollers.

Technical data

|  |  |
| --- | --- |
| Article: | CleanBox 300 |
| Model: | HEPA filter (H14) |
| Air circulation: | 100 m³/h - 300 m³/h |
| Speed controllable: | ✔ |
| Reversing capacity: | - |
| Type of voltage: | Alternating current |
| Rated voltage: | 230 V |
| Frequency: | 50 Hz/60 Hz |
| Nominal output: | 52 W |
| Imax: | 0,5 A |
| Degree of protection: | IP 20 |
| Pole-changeable: | - |
| Electrical plug-type connection: | Plug |
| Installation site: | mobile |
| Housing material: | Sheet steel, powder coated |
| Colour: | black (RAL 9005) / white (RAL 7035) |
| Weight: | 35 kg |
| Weight including packaging: | 39 kg |
| Type of filter: | Pre-filter + HEPA filter |
| Filter class: | ISO ePM1 ≥ 50 % (F7) / H14 |
| Width: | 370 mm |
| Height: | 1.168 mm |
| Depth: | 370 mm |
| Width with packaging: | 460 mm |
| Height with packaging: | 1.195 mm |
| Depth with packaging: | 400 mm |
| Ambient temperature: | -5 °C up to 40 °C |
| Sound pressure level: | 45 dB Distance 1 m, free-field conditions |
| Packing unit: | 1 piece |
| Range: | L |
| GTIN (EAN): | 4012799956495 |
| Article number: | 0095.0649 |

Manufacturer: MAICO

CleanBox 300 Air purifier